|  |  |
| --- | --- |
| Contest | Carpentry |
| Skill Performance | The contest will assess accuracy, workmanship, the ability to read and interpret blueprints, and the proper use of tools and equipment. Contestants may be required to frame walls using wood and/or steel studs; cut and install common, hip and jack rafters; and install drywall, siding, sheathing, baseboard moldings and window trim.Time limit: Contestants will be stopped when time limits, as specified on the contest job sheet, are up; however, contestants may stop whenever they have completed a particular phase of the contest.2. The dismantling of the project will be considered the final sequence or task of this contest. TBD |
| Team/Ind | Individual |
| Limits | 3 per chapter |
| Date/Location/Start Time | February 21,2020 8 A.M.Verde Valley Fair Grounds Cottonwood, Arizona |
| Attire | Dress appropriately in layers for cold weather in the morning, warming in the afternoon (weather permitting). appropriate work pants and shoes, no shorts |
| Resume | Hard copy of resume onsite is not required. |
| Chair Contact | Travis Blacktblack@vacte.com |
| Supplied by Tech Committee | a. All lumber and materials, as specified on the job sheetb. Job sheets and blueprints for each contestant and judgec. All necessary information and furnishings for judges and technical committee |
| Supplied by Contestant | a. Cut-resistant Level 3 glovesb. One 8 pt. crosscut saw (10 pt. or 12 pt. optional)c. Claw hammerd. One set chisels (1⁄4" to 1")e. Framing squaref. 16' or longer steel tape measureg. Utility knife with standard bladesh. Two pencilsi. One each — 1 and 2 pt. Phillips and 4" and 8" standard screwdrivers or one multi-tip with equivalent tipj. Wrecking bar or gooseneck pinch bark. Coping saw and extra bladel. Cat’s paw (nail puller)m. Chalk box and linen. One nail seto. Straight aviation snip or any metal cutting snipsp. 24" or 30" spirit levelq. Combination wood rasp and file (8")r. Carpenter’s tool and nail pouch with belt and/or suspenderss. Stair gaugest. Combination square and/or speed squareu. 25' power cord (UL approved grounded)v. Calculatorw. Power circular saw with new carbide tipped bladex. Drywall sawHard HatSafety Glasses |
| Other |  |