|  |  |
| --- | --- |
| Contest | Carpentry |
| Skill Performance | The contest will assess accuracy, workmanship, the ability to read and interpret blueprints, and the proper use of tools and equipment. Contestants may be required to frame walls using wood and/or steel studs; cut and install common, hip and jack rafters; and install drywall, siding, sheathing, baseboard moldings and window trim.  Time limit: Contestants will be stopped when time limits, as specified on the contest job sheet, are up; however, contestants may stop whenever they have completed a particular phase of the contest.  2. The dismantling of the project will be considered the final sequence or task of this contest. TBD |
| Team/Ind | Individual |
| Limits | 3 per chapter |
| Date/Location/Start Time | February 21,2020 8 A.M.  Verde Valley Fair Grounds  Cottonwood, Arizona |
| Attire | Dress appropriately in layers for cold weather in the morning, warming in the afternoon (weather permitting). appropriate work pants and shoes, no shorts |
| Resume | Hard copy of resume onsite is not required. |
| Chair Contact | Travis Black  tblack@vacte.com |
| Supplied by Tech Committee | a. All lumber and materials, as specified on the job sheet  b. Job sheets and blueprints for each contestant and judge  c. All necessary information and furnishings for judges and technical committee |
| Supplied by Contestant | a. Cut-resistant Level 3 gloves  b. One 8 pt. crosscut saw (10 pt. or 12 pt. optional)  c. Claw hammer  d. One set chisels (1⁄4" to 1")  e. Framing square  f. 16' or longer steel tape measure  g. Utility knife with standard blades  h. Two pencils  i. One each — 1 and 2 pt. Phillips and 4" and 8" standard screwdrivers or one multi-tip with equivalent tip  j. Wrecking bar or gooseneck pinch bar  k. Coping saw and extra blade  l. Cat’s paw (nail puller)  m. Chalk box and line  n. One nail set  o. Straight aviation snip or any metal cutting snips  p. 24" or 30" spirit level  q. Combination wood rasp and file (8")  r. Carpenter’s tool and nail pouch with belt and/or suspenders  s. Stair gauges  t. Combination square and/or speed square  u. 25' power cord (UL approved grounded)  v. Calculator  w. Power circular saw with new carbide tipped blade  x. Drywall saw  Hard Hat  Safety Glasses |
| Other |  |